**Installing Andy’s Plug (disconnect battery safely and appropriately)**

* 1. Begin by removing the driver’s seat. There are four 6mm Allen hex bolts holding the seat in place.
	2. Remove 17mm bolt securing the seat belt to the roll bar structure.
	3. Remove the plastic coverings behind the driver’s seat and pull back carpet where necessary, find the white connector plugged into the immobilizer module.
	4. Disconnect the plug.
	5. Insert Andy’s Plug into the white connector
	6. Move carpet back into place and reattach plastic covers.
	7. Use blue Loctite and reattach the seat belt to the roll bar structure.