**Immobilizer Light Deactivation (Andy’s Plug Included)**

* You can disable the immobilizer light via the factory security code method but if the key fob is used after deactivation the immobilizer will be reactivated and the fob will once again be required to start the vehicle.
* Andy’s plug negates this effect by allowing you to use the fob if you wish to do so once again at the cost of having the immobilizer light flash, but the fob will not be necessary to start the vehicle if it is used.
* All modifications are fully reversible.
* **Disarming the Alarm/Immobilizer**
* **You will need your vehicle’s security code for the immobilizer light defeat procedure (can be accessed through a Lotus dealer or owner’s manual).** The following deactivation procedure will disable the flashing LED until the fob is used again. The LED can be disabled as many times as you’d like.
	1. Turn the ignition on and off 3 times within 5 seconds.
	2. The LED will remain illuminated for a brief period indicating that the security code can now be entered, turn the ignition to the off position.
	3. You will now enter your security code. (NOTE: the number of blinks represents a digit. 5 blinks = 5)
	4. Turn ignition ON and count number of blinks representing first digit of code, then turn ignition OFF.
	5. Repeat for 2nd digit
	6. Repeat for 3rd digit
	7. Repeat for 4th digit
	8. Turn ignition ON and LED will stay illuminated (until the ignition is switched off) indicating that the correct code was entered.
* If correctly done the alarm/immobilizer LED will not flash. For verification that the procedure was done correctly, remove the key from the ignition and open then close the driver door. Reopen the door and position the key to start position (or start the vehicle); the immobilizer LED should not illuminate.
* Using the key fob will reactivate the LED however procedure 2 can be repeated to deactivate the LED once more.